Please refer to following steps for getting MG24 support in zephyr,

1. Install Zephyr related tools as per the process given in Zephyr documentation <https://docs.zephyrproject.org/latest/getting_started/index.html>
2. West workspace will be created as shown below

A picture containing icon

Description automatically generated

1. Navigate to zephyr folder

A screenshot of a computer

Description automatically generated with medium confidence

1. Delete the contents shown in step 3 and replace them with

<https://github.com/smalae/zephyr/tree/EFR32MG24_brd2601b_support>

1. Go back to workspace

A picture containing icon

Description automatically generated

1. Navigate to modules/hal/silabs

Diagram

Description automatically generated

1. Delete the contents shown in step 6 and replace them with <https://github.com/smalae/hal_silabs/tree/EFR32MG24_brd2601b_support>